aggregate scale calibration - 200
Producer	Serial No.
Type Scale
Manufacturer	Model No.
Capacity	Min. Gradation
Sensitivity	Calibration Date
Weights Added	Scale Reading	Error +	%	Weights Added	Scale Reading	Error +	%
200	5200
400	5400
600	5600
800	5800
1000	6000
1200
1400
1600
1800
2000
2200
2400
2600
2800
3000
3200
3400
3600
3800
4000
4200
4400
4600
4800
5000
Maximum Error:	Tolerance Allowed : +
Remarks: