# Mowing JSP-00-11

**1.0 Description.** This work shall consist of mowing all right of way within the construction limits of the project as approved or directed by the engineer.

**2.0 Construction Requirements.** The contractor shall be responsible for controlling the height of vegetation for traffic safety, including at approaches, crossings and intersections with abutting property to highways, railroads, trails, roads and streets.

**2.1** The contractor shall be responsible for mowing from the notice to proceed date to final acceptance of the project by the engineer. The contractor will not be responsible for mowing any section of the project where partial acceptance has been made by the engineer.

**2.2** Mowing shall be performed in a workmanlike manner with no rutting, scalping or any other resulting unsightly conditions. If mowing is determined by the engineer to be unsatisfactory, the contractor shall mow the area again at no cost to the Commission. All damaged areas shall be restored to the satisfaction of the engineer by the contractor at the contractor's expense.

**#A \*\*\*ADD THIS PARAGRAPH AS REQUIRED \*\*\***

**2.3** The contractor shall specifically be responsible for mowing XX feet [meters] left and XX feet [meters] right of the centerline from sta. XX to sta. XX. All other areas will be mowed within the limits of right of way.

**3.0 Method of Measurement.**

**3.1** Measurement of mowing will be made to the nearest 0.1 acre [0.1 ha] for the actual area mowed per mowing operation. The total quantity measured will be the summation of all of the areas approved by the engineer.

**4.0 Basis of Payment.** The accepted quantities of mowing will be paid for at the contract unit price.