# Contractor Furnished/Commission Retained Temporary Type F Concrete Traffic Barrier JSP-01-06

**1.0** **Description.** This work shall consist of providing, hauling, installing and relocating, as required, precast Temporary Type F Concrete Traffic Barrier as shown on the plans or as directed by the engineer.

**2.0 Materials.** All material shall be in accordance with Division 1000, Materials Details and Sec 617 of the Standard Specifications. No alternate barrier designs will be allowed.

**3.0 Construction Requirements.**

**3.1** Concrete barrier units placed on the project shall be new.

**3.2** The quantity of Type F barrier specified in the contract shall become the property of the Commission when no longer needed on the project and shall be hauled to the MoDOT maintenance lot at \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

**3.2.1** Delivered barrier units shall be undamaged.

**3.2.2** The contractor shall contact the District Engineer and advise the District Engineer of planned operations prior to delivering barrier units to the maintenance lot.

**3.2.3** Traffic barrier units shall be delivered to the maintenance lot to an area designated by the engineer. Traffic barrier units shall be stacked five sections per layer, three layers high, alternating the direction of each layer.

**4.0 Method of Measurement.** Measurement of Temporary Type F Concrete Traffic Barrier will be in accordance with Sec 617.6.

**5.0 Basis of Payment.** Accepted quantities of contractor furnished Temporary Type F Concrete Traffic Barrier and relocating Temporary Type F Concrete Traffic Barrier, complete in place, will be paid for at the contract unit price.

Item 617-36.02, (617-36.03), Contractor Furnished/Commission Retained Temporary

Type F Concrete Traffic Barrier

Item 617-50.10 (617-50.15), Relocating Temporary Traffic Barrier