# Winter Months Requirements JSP-15-07A

1. **Description.** This project contains work which spans the winter months.
2. **Work to be Completed.** When the contractor ceases operations for the winter months, any paving operation performed by the contractor shall not result in a lane height differential between adjacent lanes.
3. **Maintenance of Pavement Marking.** Prior to ceasing operations for winter months, a permanent or temporary stripe shall be provided on any completed length to the point that the original stripe was obliterated or obscured by the contractors’ operation. Temporary striped areas shall be re-striped with the remaining route upon performance of the final striping.
4. **Winter Related Maintenance Activities.** The contractor shall have the project in a condition as not to interfere with the plowing of snow. The contractor shall also provide a taper at the end of his paving that will not be damaged by the plowing of snow.
5. **Basis of Payment.** There will be no direct pay for compliance with this provision.