


Construction Vehicle Warning System JSP-26-02

INCLUDE WORK ZONE INTELLIGENT TRANSPORTATION SYSTEM (NJSP1532), WHEN USING THIS JSP.

AT LEAST ONE (1) “TRUCKS ENTERING ROADWAY” STATIC SIGN AND CHANGEABLE MESSAGE BOARD WILL NEED TO BE ADDED TO THE CONTRACT TO FACILITATE THE DEPLOYMENT OF THIS JSP.

1.0  General  The Construction Vehicle Warning System (CVWS) is a portable, automated, and real-time Work Zone Intelligent Transportation System (WZITS) subsystem that displays warning messages to oncoming regular traffic when slow-moving construction vehicles are merging into regular traffic.

2.0  Description  This item shall consist of furnishing, installing, relocating, operating, and removing a portable, automated real-time CVWS meeting the requirements in these provisions.

3.0  System Requirements  The CVWS shall include portable changeable message signs (CMS), static “Trucks Entering Roadway” signs, WZITS Traffic Sensors, and appropriate hardware and/or software to detect construction vehicles that will re-enter highway traffic flow, from the work zone.  The CMS shall be in accordance with Sec 616.  Detection of approaching regular traffic is not required.

3.1  The contractor shall relocate the device as directed by the engineer.  When the equipment is no longer required for this project, the contractor shall remove it and retain ownership.

3.2  The CVWS shall remain operational and detect all construction vehicle traffic entering regular traffic, 24 hours per day, seven days per week.

3.3  The CMS shall be visible, legible and begin displaying a warning message 4 to 8 seconds prior to the construction vehicle entering the regular travel lane.

4.0  Work Zone Intelligent Transportation System Plan.  In addition to the WZITS Plan required in Sec 616.11 and the WZITS provision, the CVWS section shall include the following items:

· The proposed locations of proposed field devices, for each phase of construction.
· A description of message activation logic and proposed CMS messages.
· A detailed description of the proposed methods of communication between system components.

5.0  System Performance.  The contractor shall furnish all labor and materials to provide a functional system, as described in these provisions, including the installation, maintenance, and operation of field equipment. The performance of the field equipment shall not be degraded by number of lanes of travel, visibility conditions, roadway conditions, or inclement weather, including precipitation, fog, darkness, excessive dust, or road debris.

6.0  Basis of Payment.  Payment for furnishing, installing, relocating, operating, maintaining, testing, monitoring, and removal of the CVWS will be covered by the contract unit price for Item Number 616-99.01, “Construction Vehicle Warning System” per lump sum. Required CMS boards and static sign assemblies will be included in the cost of 616-10.05 Construction Signs (SF) or 616-99.01 Lump Sum Traffic Control depending on the contract, additional CMS boards and static sign assemblies which will be paid separately.





