##. SAFETY REQUIREMENTS

**[DRAFTERS NOTE: This JSP is only required on projects within MoDOT Right of Way]**

**Delete Sec 616.3.1 and substitute the following:**

**616.3.1** All workers within MoDOT right of way shall wear approved ANSI/ISEA 107 Performance Class 2 or 3 safety apparel and more specifically as follows:

**616.3.1.1 Daytime Flagger**. During daytime activities, flaggers shall wear a high visibility hard hat, safety glasses, a Performance Class 3 top OR a Performance Class 2 top, and safety footwear. Hard hats other than high visibility orange or green shall be covered with a high visibility covering.

**616.3.1.2 Daytime Worker**. During daytime activities, workers shall wear a hard hat, safety glasses, a Performance Class 3 top OR a Performance Class 2 top, and safety footwear.

**616.3.1.3 Nighttime Flagger**. During nighttime activities, flaggers shall wear a high visibility/reflective hard hat, safety glasses, a Performance Class 3 top AND Class E bottoms, OR Performance Class 2 top AND Class E bottoms, and safety footwear. Hard hats shall be reflective or covered with a high visibility covering.

**616.3.1.4 Nighttime Worker**. During nighttime activities, workers shall wear a hard hat, safety glasses, a Performance Class 3 top OR Performance Class 2 top AND Class E bottoms, and safety footwear.

Note: A graphic representation of the various PPE as described above can be found in the “Additional Information” portion of these provisions. A color representation can be found on the MoDOT website at: <http://tinyurl.com/Safe-Apparel>.