# Placing State-Owned Pipe JSP-04-08

**1.0 Description.** This work shall consist of laying State-owned pipe or pipe-arch culverts at locations directed by the engineer.

**2.0 Construction Requirements.** State-owned pipe shall be laid in accordance with the requirements for placing new pipe, except that the pipe and all necessary coupling bands will be furnished at the job site by the Commission at no cost to the contractor. Excavation for removal of the pipe will not be required.

**3.0 Method of Measurement.**

**3.1** Measurement of placing State-owned pipe will be made to the nearest linear foot (0.5 m) along the geometrical center of the pipe in place.

**3.2** Measurement of Class 3 Excavation for placing the pipe will be made in accordance with Sec 206.

**4.0 Basis of Payment.**

**4.1** Payment for placing State-owned pipe will be made per linear foot (meter) at the fixed unit price specified in Sec 109.14. Payment for placing pipe-arch will be at the rate for circular pipe from which the arch was developed.

**4.2** Payment for Class 3 Excavation for placing the pipe will be made at the contract unit price per cubic yard (cubic meter) under roadway items.

**4.3** No direct payment will be made for any required hauling, cutting, joining or backfilling of the pipe.