PROJECT DATA FOR BAMS

Program Job No. *

Contract Number: [A]

Project Number: [A]

Primary County Number: (c3) Primary District Number: (c2)

Secondary County Number: (c3) Type of Work: (c7) [B]

Consultant Design Bridge Roadway Both [A]

Project Length:

Item Specification Year: (c2)

Beg. Sta. or Log Mi.: (c20)	Designed by: (c20)

End Sta. or Log Mi.: (c20)	Estimated by: (c20)

[C]	X Coord. of Project Midpt.: Y Coord. of Project Midpt.:

(Longitude) Deg.,Min.,Sec. (Latitude) Deg.,Min.,Sec.

[A]	To be completed by Headquarters.

[B]	Fill in appropriate work category - see back of sheet for categories

[C]	Entry required for longitude and latitude (may be obtained from county map or USGS map - enter in degrees minutes and seconds - if seconds are not known enter as "00")

(c13)	c indicates character - may be letters or numbers

13 indicates number of characters allowed

*	Leveling course jobs should be identified by using the program job number plus a number (1 thru 99) for each project within the job number. For example J1S0488D3. This number should be shown on the estimate header sheet.

TYPES OF WORK

1	2	3	4	5	6	7

Design Type (1)

R - Rural or U - Urban (population > 50,000)

Construction Traffic (2)

N - None -- Job on relocation or route closed	M - Medium -- 400-1700 ADT

L - Light -- 0-400 ADT	H - Heavy -- over 1700 ADT

Description of Project (5-7)	Description of Major Work Involved (3-4)

CON	01.	Grading and drainage (paving to be done later)

CON	02.	Grading, drainage, and bridge

CON	03.	Grading, drainage, and paving

CON	04.	Grading, drainage, bridge, and paving

PCC	05.	Concrete pavement

PCC	06.	Concrete resurfacing

ASP	07.	Asphalt paving (initial paving)

ASP	08.	Asphalt & Bituminous Resurf. (except level course)

ASP	09.	Widening (6' or less per side) and resurfacing

ASP	10.	Level course work

REH	11.	Pavement Repair Only

ASP	12.	Cold Milling and Resurfacing

BRG	21.	Bridge (new)

BRG	22.	Bridge (rehab.)

BRG	23.	Bridge painting

BRG	24.	Bridge removal

BRG	25.	Bridge strengthening

BRG	26.	Bridge joint repair and overlay

SAF	30	Slide corrections

SAF	35	Signals

SAF	40	Guardrail

SAF	45	Signing

SAF	50	Delineators

SAF	55	Lighting

BLD	60	Weigh Stations

BLD	65.	Rest areas

REH	70	Widen and stabilize shoulder

AVI	75	Aviation

MIS	99	Miscellaneous - not covered by any of above

Note: To determine type of work, choose the correct values for the following and place in the appropriate block under TYPES OF WORK: design type-1, construction traffic-2, description of major work involved-3 and 4, and description of project-5, 6, and 7. For example, a project involving signals in a light, rural setting would be coded as RL35SAF.